Non-Compliant

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade Model 2050

SPECfp_rate2000 = SPECfp_rate_base2000 = NC NC SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Nov-2001 Hardware Avail: Feb-2002 Software Avail: Feb-2002

SPEC has determined that this result was not in compliance with the SPEC CPU2000 run and reporting rules. Specifically, the original tester has discovered that performance of the final system changed by more than 1.75% versus the tested system, and has requested that this result be marked non-compliant. Replacement results can be found at: http://www.spec.org/cpu2000/results/res2002q2/cpu2000-20020422-01316.asc

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 1 2 3 4 5 168.wupwise 2 NC NC 2 NC NC

171.swim 2 NC NC 2 NC NC

172.mgrid 2 NC NC 2 NC NC

173.applu 2 NC NC 2 NC NC

177.mesa 2 NC NC 2 NC NC

178.galgel 2 NC NC 2 NC NC

179.art 2 NC NC 2 NC NC

183.equake 2 NC NC 2 NC NC

187.facerec 2 NC NC 2 NC NC

188.ammp 2 NC NC 2 NC NC

189.lucas 2 NC NC 2 NC NC

191.fma3d 2 NC NC 2 NC NC

200.sixtrack 2 NC NC 2 NC NC

301.apsi 2 NC NC 2 NC NC

Hardware

CPU: UltraSPARC III Cu CPU MHz: 1050 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 8GB Disk Subsystem: 2 x 73GB Other Hardware: None

Software

Operating System: Solaris 8 10/01 Compiler: Forte Developer 7 EA File System: tmpfs System State: Multi-User

Notes/Tuning Information

Portability:
 178.galgel: -e -fixed

Base Flags:
 Base C flags: -fast -xipo=2 -xalias_level=std -xprofile

Non-Compliant

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade Model 2050

SPECfp_rate2000 = SPECfp_rate_base2000 = NC NC SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Nov-2001 Hardware Avail: Feb-2002 Software Avail: Feb-2002

SPEC has determined that this result was not in compliance with the SPEC CPU2000 run and reporting rules. Specifically, the original tester has discovered that performance of the final system changed by more than 1.75% versus the tested system, and has requested that this result be marked non-compliant. Replacement results can be found at: http://www.spec.org/cpu2000/results/res2002q2/cpu2000-20020422-01316.asc

Notes/Tuning Information (Continued)

 Base F90 flags: -fast -xcrossfile -lprism32 -xprofile

Peak Flags:
 168.wupwise: basepeak=yes
 171.swim: basepeak=yes
 172.mgrid: basepeak=yes
 173.applu: -fast -Qoption iropt -Adata_access,-Mt7000,-Mm14000,-Mr40000,-Ma400,-whole
            -xregs=syst -Qoption iropt -Rscalarrep,-MR -Qoption cg -Qlp=1-av=192-fa=1
            -Qoption f90comp -O3
 177.mesa: -fast -xcrossfile -xalias_level=strong -xprofile
 178.galgel: -fast -xcrossfile -xregs=syst -Qoption iropt -Addint:sf=9 -lsunperf -xprofile
 179.art: basepeak=yes
 183.equake: -fast -xalias_level=strong -xdepend -W2,-whole,-Amemopt:arrayloc -xprefetch
             -Wc,-Qms_pipe-pref,-Qlp=1-av=256-t=4-fa=1-fl=1 -lprism32 -lmopt -xprofile
 187.facerec: basepeak=yes
 188.ammp: -fast -xcrossfile -xalias_level=std -lprism32 -xprofile
 189.lucas: -fast -Qoption f90comp -array_pad_rows,2002 -Qoption iropt -whole
            -xdepend -xprefetch -Qoption cg -Qms_pipe-pref,-Qlp=1-t=3-fa=1
            -lprism32 -xprofile
 191.fma3d: -fast -xcrossfile -stackvar -xdepend -xprefetch
            -Qoption cg -Qlp=1-av=256-t=3-fa=1 -xprofile
 200.sixtrack: basepeak=yes
 301.apsi: -fast -Qoption iropt -Mt450 -lprism32 -xprofile

Forte Developer 7 EA (Early Access) will ship by Feb-2002
Forte Developer 7 (final) will ship May-2002

ONESTEP=yes for all benchmarks in peak and Fortran benchmarks in base

Shell Environments:
 LD_LIBRARY_PATH=/usr/lib:/opt/fd7/lib/v8plusb:/opt/fd7/YNH/lib/v8plusb
 PRISM_HEAP=268435456
 PRISM_MODE=2

 Stack size set to unlimited via "ulimit -s unlimited"

Kernel Parameters (/etc/system):
 set shmsys:shminfo_shmmin=1
 set shmsys:shminfo_shmmax=1477846784
 set shmsys:shminfo_shmmni=256
 set shmsys:shminfo_shmseg=400

System configuration details located (as of Nov 2001) at
     http://www.sun.com/desktop/products/ws.html