Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 2900 Cu

SPECfp_rate2000 = SPECfp_rate_base2000 =

14.9 12.6

SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Nov-2001 Hardware Avail: Dec-2001 Software Avail: Feb-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 50 100 150 200 250 168.wupwise 2 299 12.4 2 299 12.4

171.swim 2 555 13.0 2 555 13.0

172.mgrid 2 490 8.52 2 490 8.52

173.applu 2 861 5.66 2 404 12.1

177.mesa 2 297 10.9 2 289 11.2

178.galgel 2 205 32.8 2 164 41.1

179.art 2 31.8 190 2 31.8 190

183.equake 2 247 12.2 2 157 19.2

187.facerec 2 239 18.4 2 239 18.4

188.ammp 2 519 9.83 2 506 10.1

189.lucas 2 963 4.82 2 493 9.41

191.fma3d 2 654 7.45 2 619 7.87

200.sixtrack 2 357 7.16 2 357 7.16

301.apsi 2 729 8.27 2 648 9.31

Hardware

CPU: UltraSPARC III Cu CPU MHz: 900 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1-2 Parallel: None Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 2GB Disk Subsystem: 1 x 36GB Other Hardware: --

Software

Operating System: Solaris 8 10/01 Compiler: Forte Developer 7 EA File System: tmpfs System State: Multi-User

Notes/Tuning Information

Portability:
 178.galgel: -e -fixed

Base Flags:
 Base C flags: -fast -xipo=2 -xalias_level=std -xprofile
 Base F90 flags: -fast -xcrossfile -lprism32 -xprofile

Peak Flags:
 168.wupwise: basepeak=yes
 171.swim: basepeak=yes
 172.mgrid: basepeak=yes
 173.applu: -fast -Qoption iropt -Adata_access,-Mt7000,-Mm14000,-Mr40000,-Ma400,-whole
            -xregs=syst -Qoption iropt -Rscalarrep,-MR -Qoption cg -Qlp=1-av=192-fa=1
            -Qoption f90comp -O3
 177.mesa: -fast -xcrossfile -xalias_level=strong -xprofile
 178.galgel: -fast -xcrossfile -xregs=syst -Qoption iropt -Addint:sf=9 -lsunperf -xprofile

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 2900 Cu

SPECfp_rate2000 = SPECfp_rate_base2000 =

14.9 12.6

SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Nov-2001 Hardware Avail: Dec-2001 Software Avail: Feb-2002

Notes/Tuning Information (Continued)

 179.art: basepeak=yes
 183.equake: -fast -xalias_level=strong -xdepend -W2,-whole,-Amemopt:arrayloc -xprefetch
             -Wc,-Qms_pipe-pref,-Qlp=1-av=256-t=4-fa=1-fl=1 -lprism32 -lmopt -xprofile
 187.facerec: basepeak=yes
 188.ammp: -fast -xcrossfile -xalias_level=std -lprism32 -xprofile
 189.lucas: -fast -Qoption f90comp -array_pad_rows,2002 -Qoption iropt -whole
            -xdepend -xprefetch -Qoption cg -Qms_pipe-pref,-Qlp=1-t=3-fa=1
            -lprism32 -xprofile
 191.fma3d: -fast -xcrossfile -stackvar -xdepend -xprefetch
            -Qoption cg -Qlp=1-av=256-t=3-fa=1 -xprofile
 200.sixtrack: basepeak=yes
 301.apsi: -fast -Qoption iropt -Mt450 -lprism32 -xprofile

Forte Developer 7 (final) will ship May-2002

ONESTEP=yes for all benchmarks in peak and Fortran benchmarks in base

Shell Environments:
 LD_LIBRARY_PATH=/usr/lib:/opt/fd7/lib/v8plusb:/opt/fd7/YNH/lib/v8plusb
 PRISM_HEAP=268435456
 PRISM_MODE=2

 Stack size set to unlimited via "ulimit -s unlimited"

Kernel Parameters (/etc/system):
 set shmsys:shminfo_shmmin=1
 set shmsys:shminfo_shmmax=1477846784
 set shmsys:shminfo_shmmni=256
 set shmsys:shminfo_shmseg=400

System configuration details located (as of Dec 2001) at
     http://www.sun.com/desktop/products/ws.html