Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation c3650

SPECfp_rate2000 = SPECfp_rate_base2000 =

6.29 5.59

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Dec-2001 Hardware Avail: Nov-2001 Software Avail: Jan-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 2 4 6 8 10 12 14 16 168.wupwise 1 471 3.94 1 282 6.58

171.swim 1 338 10.6 1 338 10.6

172.mgrid 1 342 6.11 1 342 6.11

173.applu 1 333 7.31 1 333 7.31

177.mesa 1 353 4.60 1 349 4.65

178.galgel 1 223 15.1 1 223 15.1

179.art 1 450 6.70 1 297 10.2

183.equake 1 353 4.27 1 255 5.92

187.facerec 1 566 3.90 1 551 4.00

188.ammp 1 505 5.05 1 433 5.89

189.lucas 1 529 4.39 1 503 4.61

191.fma3d 1 655 3.72 1 639 3.81

200.sixtrack 1 326 3.92 1 289 4.42

301.apsi 1 479 6.30 1 479 6.30

Hardware

CPU: PA-8700 CPU MHz: 625 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 0.75MB(I) + 1.5MB(D) on chip Secondary Cache: None L3 Cache: None Other Cache: None Memory: 2GB (4x512MB DIMMs) Disk Subsystem: 1x18 GB SCSI Other Hardware:

Software

Operating System: HP-UX 11i TCOE B.11.11.0109 PHKL_24779 LVM Cumulative Patch Compiler: HP ANSI C B11.11.04 Fortran90 B11.11.47 PHSS_24207 libm patch File System: VxFS System State: Multi-user

Notes/Tuning Information

  Portability flags:
   178.galgel: +source=fixed

 Baseline compile flags:
   fortran: +O3 +Onofltacc -Wl,-a,archive -Wl,+FPD
   C      : +I/+P +O4 +Odataprefetch -Wl,-a,archive

 Peak compile flags:
   168.wupwise: (ONESTEP) +cat +O3 +Odataprefetch +Onofltacc
                -Wl,+FPD -Wl,-a,archive
   171.swim: basepeak=true
   172.mgrid: basepeak=true
   173.applu: basepeak=true
   177.mesa: +I/+P +Oall +Odataprefetch +Opromote_indirect_calls
             -Wl,+FPD -Wl,-a,archive
   178.galgel: basepeak=true

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation c3650

SPECfp_rate2000 = SPECfp_rate_base2000 =

6.29 5.59

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Dec-2001 Hardware Avail: Nov-2001 Software Avail: Jan-2002

Notes/Tuning Information (Continued)

   179.art: +I/+P +Oall +Onodataprefetch +Onofltacc +Optrs_strongly_typed
            +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   183.equake: +O4 +Olibcalls +Odataprefetch +Optrs_strongly_typed
               +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   187.facerec: (ONESTEP) +cat +O3 +Ofastaccess -Wl,+FPD -Wl,-a,archive
   188.ammp: +I/+P +Oall +Odataprefetch +Optrs_strongly_typed
             +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   189.lucas: +O3 +Onoinline -Wl,+FPD -Wl,-a,archive
   191.fma3d: +O3 +Onolimit -Wl,+FPD -Wl,-a,archive
   200.sixtrack: (ONESTEP) +cat +O3 +Onolibcalls +Onolimit +Onoinline
                 +Onodataprefetch -Wl,+FPD -Wl,-a,archive
   301.apsi: basepeak=true

 Operating system configuration notes:

   vps_pagesize 4096, vps_ceiling 16384
   dbc_min_pct 15, dbc_max_pct 15
   maxdsiz 0x7b03a000, maxssiz 256000000
   nfile 8192