Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp carrier grade server cc2300

SPECint2000 = SPECint_base2000 = 550 541 SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Jan-2002 Hardware Avail: Mar-2002 Software Avail: Dec-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 300 600 900 1200

164.gzip 1400 201 695 201 697

175.vpr 1400 300 466 300 467

176.gcc 1100 171 644 173 637

181.mcf 1800 591 305 592 304

186.crafty 1000 152 656 153 653

197.parser 1800 372 484 372 484

252.eon 1300 302 430 253 515

253.perlbmk 1800 261 689 260 693

254.gap 1100 214 514 213 515

255.vortex 1900 234 811 234 813

256.bzip2 1500 303 495 303 495

300.twolf 3000 590 508 581 517

Hardware

CPU: Pentium III processor (1263 MHz, 133 MHz bus) CPU MHz: 1263 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1-2 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 768 MB (6 128 MB SDRAM 133 MHz DIMMs) Disk Subsystem: One 18 GB Ultra3 10K rpm disk (HP A6917A) Other Hardware: None

Software

Operating System: RedHat Linux 7.1 Compiler: Intel C/C++ Compiler 5.0.1 for Linux RH 7.1 (Build 011112D0) File System: Default System State: Default

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use
 Base tuning for C programs:   -xK -ipo -fp_port +FDO
 Base tuning for C++ programs: -xK -fp_port -Kc++eh -Krtti
 Portability flags:
 176.gcc:     -Dalloca=_alloca -DUSG
 186.crafy:   -DLINUX_i386
 253.perlbmk: -DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL -DSPEC_CPU2000_GLIBC22
 253.perlbmk: src.alt for glibc 2.2 used
 254.gap:     -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
 254.gap:     -DSYS_HAS_SIGNAL_PROTO _DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
 Peak tuning:
 164.gzip, 175.vpr, 176.gcc, 181.mcf, 186.crafty, 197.parser
 253.perlbmk, 254.gap, 300.twolf:
 -xK -ipo +FDO
 255.vortex, 256.bzip2:
 -xK -ipo +FDO -Oa
 252.eon:
 -xK -ipo +FDO -O3