Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell PowerEdge 4400 (1.0 GHz PIII Xeon)

SPECfp2000 = SPECfp_base2000 = 317 302 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Oct-2001 Hardware Avail: May-2001 Software Avail: Jun-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500 600

168.wupwise 1600 400 400 397 403

171.swim 3100 963 322 913 340

172.mgrid 1800 827 218 799 225

173.applu 2100 862 243 851 247

177.mesa 1400 258 544 254 552

178.galgel 2900 782 371 741 391

179.art 2600 783 332 833 312

183.equake 1300 651 200 450 289

187.facerec 1900 506 375 499 381

188.ammp 2200 736 299 727 303

189.lucas 2000 667 300 649 308

191.fma3d 2100 661 318 640 328

200.sixtrack 1100 668 165 667 165

301.apsi 2600 790 329 715 364

Hardware

CPU: Intel PentiumIII Xeon CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 16KB(I) + 16KB(D) on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4GB (8 x 512MB SDRAM) Disk Subsystem: 1 x 18GB Seagate Ultra-III Other Hardware:

Software

Operating System: Windows 2000 Server (SP2) Compiler: Intel C++ and Fortan Compiler 5.0.1 (010727Z)

Microsoft Visual C++ 6.0 (SP5) MicroQuill SmartHeap Library 5.0

File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY
   178.galgel:   -FI /F32000000
 FEEDBACK-DIRECTED OPTIMIZATION
   FDO:         PASS1= /Qprof_gen  PASS2= /Qprof_use
 BASE TUNING
   C/F77/F90:    /Qipo +FDO /QxK /O3
 PEAK TUNING
   168.wupwise:  /Qipo +FDO /QxK /O3
   171.swim:     /Qipo +FDO /QxK /O3
   172.mgrid:    /Qipo +FDO /QaxK /O3
   173.applu:    /Qipo +FDO /QxK /O3
   177.mesa:     -Qipo +FDO -QxK -O3 -Oa shlW32M.lib
   178.galgel:   /Qipo +FDO /QxK /O3 shlW32M.lib
   179.art:      -Qipo +FDO -QxK -O3 shlW32M.lib
   183.equake:   -Qipo +FDO -QxK -Qrcd -Oa shlW32M.lib
   187.facerec:  /Qipo +FDO /QxK /O3 shlW32M.lib
   188.ammp:     -Qipo +FDO -QxK -O3 -Oa

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell PowerEdge 4400 (1.0 GHz PIII Xeon)

SPECfp2000 = SPECfp_base2000 = 317 302 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Oct-2001 Hardware Avail: May-2001 Software Avail: Jun-2001

Notes/Tuning Information (Continued)

   189.lucas:    /Qipo +FDO /QxK /O3 shlW32M.lib
   191.fma3d:    /Qipo +FDO /QxK /O3
   200.sixtrack: /Qipo +FDO /QxK /O3
   301.apsi:     /Qipo +FDO /QxK
 EXTRA LIBRARIES
   shlW32M.lib:  MicroQuill SmartHeap Library 5.0
                 www.microquill.com
 LIBRARY ORDERING
   178.galgel, 187.facerec, 189.lucas:
                 libIEPCF90.lib libintrins.lib libF90.lib libqwin.lib
                 libm.lib shlW32M.lib LIBC.lib libirc.lib OLDNAMES.lib
 /numprocs=1 was added to c:�oot.ini file to disable additional CPUs on this system