Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 150 (650 MHz)

SPECfp2000 = SPECfp_base2000 = 276 261 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Aug-2002 Hardware Avail: Aug-2002 Software Avail: Aug-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 300 600 900 1200

168.wupwise 1600 497 322 497 322

171.swim 3100 1399 222 1399 222

172.mgrid 1800 1103 163 1103 163

173.applu 2100 1428 147 978 215

177.mesa 1400 440 318 440 318

178.galgel 2900 896 324 745 389

179.art 2600 255 1019 255 1019

183.equake 1300 444 292 413 315

187.facerec 1900 617 308 617 308

188.ammp 2200 1103 199 941 234

189.lucas 2000 873 229 857 233

191.fma3d 2100 1057 199 1057 199

200.sixtrack 1100 490 224 490 224

301.apsi 2600 1286 202 1305 199

Hardware

CPU: UltraSPARC IIi CPU MHz: 650 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 16KBI+16KBD on chip Secondary Cache: 512KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 256MB Disk Subsystem: 1 x Seagate ST340016A Other Hardware: None

Software

Operating System: Solaris 8 2/02 Compiler: Sun ONE Studio 7 and Sun Performance Library 7 File System: ufs System State: Multi-User

Notes/Tuning Information

Portability:
 178.galgel: -e -fixed

Profile Feedback (-xprofile):
       fdo_pre0: rm -rf ./feedback.profile ./SunWS_cache
         Pass 1: -xprofile=collect:./feedback
         Pass 2: -xprofile=use:./feedback
Base Flags:
 Base C   flags: -fast -xipo=2 -xalias_level=std -xprofile
 Base F90 flags: -fast -xcrossfile -xprofile

Peak Flags:
    168.wupwise: basepeak=yes
       171.swim: basepeak=yes
      172.mgrid: basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 150 (650 MHz)

SPECfp2000 = SPECfp_base2000 = 276 261 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Aug-2002 Hardware Avail: Aug-2002 Software Avail: Aug-2002

Notes/Tuning Information (Continued)

      173.applu:  -fast -xchip=ultra3 -Qoption iropt -Adata_access,-Mt7000,-Mm14000,-Mr40000,-Ma400,-whole

                  -xregs=syst -Qoption iropt -Rscalarrep,-MR -Qoption cg
                  -Qlp=1-av=192-fa=1 -Qoption f90comp -O3 -xprofile
       177.mesa: basepeak=yes

     178.galgel: -fast -xcrossfile -xregs=syst -Qoption iropt -Addint:sf=9 -xlic_lib=sunperf -lsunperf -xprofile

        179.art: basepeak=yes
     183.equake: -fast -xchip=ultra3 -xipo=2 -xalias_level=std -lmopt -xprofile
     187.facerec: basepeak=yes
       188.ammp: -fast -xchip=ultra3 -xcrossfile -xalias_level=std -xprofile
      189.lucas: -fast -xchip=generic -xcrossfile -Qoption cg -Qms_pipe=a -xprofile
      191.fma3d: basepeak=yes
   200.sixtrack: basepeak=yes
       301.apsi: -fast -Qoption iropt -Mt450 -xprofile
ONESTEP=yes for all benchmarks except 179.art in peak
ONESTEP=yes for Fortran benchmarks in base

 Stack size set to unlimited via "ulimit -s unlimited"

Software Patches: All patches for the Sun ONE Studio 7 Compiler (Product Patches and
OS patches) as recommended by http://access1.sun.com/sundev/s1s7-patches.html on Aug
the 7th, 2002 were installed (111704-03 111705-02 111706-01 111708-01 111709-01
111714-01 111715-01 111716-02 111718-01 111723-01 108434-08 108435-08 111697-03
111721-02)