Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 530 (2.4 GHz Xeon)} SPECfp2000 =

SPECfp_base2000 = 827 821 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Sep-2002 Hardware Avail: Apr-2002 Software Avail: Jun-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 151 1063 144 1109

171.swim 3100 232 1335 232 1335

172.mgrid 1800 234 770 234 771

173.applu 2100 247 849 243 864

177.mesa 1400 153 913 152 918

178.galgel 2900 250 1160 250 1160

179.art 2600 476 546 475 547

183.equake 1300 135 962 140 927

187.facerec 1900 183 1038 183 1038

188.ammp 2200 456 483 454 485

189.lucas 2000 178 1125 172 1165

191.fma3d 2100 257 817 257 817

200.sixtrack 1100 259 424 251 438

301.apsi 2600 415 626 413 630

Hardware

CPU: Intel Xeon (400 MHz system bus) CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2 x 256MB PC800-45 ECC RDRAM Disk Subsystem: 1 x 18GB Fujitsu Limited 10K U160 Other Hardware:

Software

Operating System: Windows XP Professional Compiler: Intel C++ and Fortan Compiler 6.0 (020423Z)

Microsoft Visual Studio .NET (7.0.9466) MicroQuill SmartHeap Library 6.01

File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY
   178.galgel:   -FI -F32000000
 FEEDBACK-DIRECTED OPTIMIZATION
   FDO:          PASS1= -Qprof_gen  PASS2= -Qprof_use
 BASE TUNING
   C-F77-F90:    -Qipo -QxW -O3 +FDO
 PEAK TUNING
   168.wupwise:  -Qipo -QxW +FDO
   171.swim:     -Qipo -QxW -O3 +FDO
   172.mgrid:    -Qipo -QaxW -O3 +FDO
   173.applu:    -Qipo -QxW -O3 -Qscalar_rep- +FDO
   177.mesa:     -Qipo -QxW -O3 -Oa +FDO
   178.galgel:   -Qipo -QxW -O3 +FDO
   179.art:      -Qipo -QxW -O3 -Oa +FDO
   183.equake:   -Qipo -QxW -O3 -Oa +FDO shlW32M.lib
   187.facerec:  -Qipo -QxW -O3 +FDO
   188.ammp:     -Qipo -QxW -O3 -Oa +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 530 (2.4 GHz Xeon)} SPECfp2000 =

SPECfp_base2000 = 827 821 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Sep-2002 Hardware Avail: Apr-2002 Software Avail: Jun-2002

Notes/Tuning Information (Continued)

   189.lucas:    -Qipo -QaxW
   191.fma3d:    -Qipo -QxW -O3 +FDO
   200.sixtrack: -Qipo -QxW +FDO
   301.apsi:     -Qipo -QxW +FDO
 EXTRA LIBRARIES
   shlW32M.lib:  MicroQuill SmartHeap Library 6.01
                 www.microquill.com