Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V65x (3.06 GHz Xeon)

SPECfp2000 = SPECfp_base2000 =

1011 1010

SPEC license #: 6 Tested by: Sun Microsystems Test date: Apr-2003 Hardware Avail: May-2003 Software Avail: Apr-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 125 1285 125 1285

171.swim 3100 212 1460 212 1460

172.mgrid 1800 189 954 188 956

173.applu 2100 207 1014 207 1014

177.mesa 1400 103 1353 103 1353

178.galgel 2900 194 1498 194 1498

179.art 2600 383 679 383 679

183.equake 1300 105 1236 105 1238

187.facerec 1900 149 1271 149 1271

188.ammp 2200 398 553 398 553

189.lucas 2000 161 1242 161 1242

191.fma3d 2100 202 1041 202 1041

200.sixtrack 1100 201 548 198 555

301.apsi 2600 350 743 350 743

Hardware

CPU: Intel Xeon (533MHz system bus) CPU MHz: 3066 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: None Other Cache: None Memory: 2GB (2 x 1GB) Disk Subsystem: 1 x 36GB Seagate Ultra320 SCSI Other Hardware: None

Software

Operating System: Red Hat Linux 7.3 Compiler: Intel(R) Fortran Compiler for 32-bit applications

Version 7.1 Build 20030402Z Intel(R) C++ Compiler for 32-bit applications Version 7.1 Build 20030307Z Microquill SmartHeap 6.02

File System: ext2 System State: Multi-User (run level 3), hyperthreading disabled in BIOS

Notes/Tuning Information

Portability:
 178.galgel: -FI

Profile Feedback (+FDO):
 rm -rf ‘pwd‘/*.dyn ‘pwd‘/*.dpi ‘pwd‘/*.il
 Pass 1: -prof_gen
 Pass 2: -prof_use

Base Flags:
 Base tuning: -xW -ipo -O3 +FDO

Peak Flags:
 168.wupwise: basepeak=yes
 171.swim: basepeak=yes
 172.mgrid: -ipo -xW -O3 -L${SH_PATH} -lsmartheap +FDO
 172.mgrid: (SH_PATH is the path to the SmartHeap library)

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V65x (3.06 GHz Xeon)

SPECfp2000 = SPECfp_base2000 =

1011 1010

SPEC license #: 6 Tested by: Sun Microsystems Test date: Apr-2003 Hardware Avail: May-2003 Software Avail: Apr-2003

Notes/Tuning Information (Continued)

 173.applu: basepeak=yes
 177.mesa: basepeak=yes
 178.galgel: basepeak=yes
 179.art: basepeak=yes
 183.equake: -ipo -xW -rcd -O3 +FDO
 187.facerec: basepeak=yes
 188.ammp: basepeak=yes
 189.lucas: basepeak=yes
 191.fma3d: basepeak=yes
 200.sixtrack: -ipo -xW +FDO
 301.apsi: basepeak=yes
 2nd processor physically removed