Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant BL20p G2 (3.06GHz/1MB L3 cache, Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1193 1160

SPEC license #: 3 Tested by:Hewlett-Packard Company, Houston TX Test date: Aug-2003 Hardware Avail: Jul-2003 Software Avail: Jun-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 111 1444 113 1419

171.swim 3100 196 1582 185 1676

172.mgrid 1800 153 1180 151 1193

173.applu 2100 190 1104 188 1116

177.mesa 1400 112 1248 112 1248

178.galgel 2900 165 1761 164 1772

179.art 2600 286 908 270 963

183.equake 1300 113 1155 90.8 1432

187.facerec 1900 131 1445 130 1460

188.ammp 2200 240 917 238 924

189.lucas 2000 142 1407 141 1415

191.fma3d 2100 185 1137 185 1137

200.sixtrack 1100 197 559 192 573

301.apsi 2600 264 986 263 988

Hardware

CPU: Intel Xeon (3.06GHz, 533MHz bus) CPU MHz: 3066 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K micro-ops I + 8KBD on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: 1024KB(I+D) on chip Other Cache: N/A Memory: 2x1024MB PC2100 Disk Subsystem: 2x18.2GB 15K Ultra3 SCSI Other Hardware:

Software

Operating System: Windows 2000 Server (Build 2195 SP3) Compiler: Intel C++ Compiler 7.1 Build 20030801Z

Microsoft Visual Studio Enterprise Edition 6.0 (for libraries) Intel Fortran Compiler 7.1 build 20030307Z MicroQuill Smartheap Library 7.0

File System: NTFS System State: Hyperthreading disabled in BIOS

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning: -QxW -Qipo -O3 +FDO ONESTEP=yes
 Portability:
 178.galgel: -FI /F32000000
 Peak tuning:
 168.wupwise:    -Qipo -QxW  +FDO ONESTEP=yes
 171.swim:       -Qipo -QxW  -O3 +FDO ONESTEP=yes
 172.mgrid:      -Qipo -QaxW -O3 +FDO ONESTEP=yes
 173.applu:      -Qipo -QxW  -O3 -Qscalar_rep- +FDO ONESTEP=yes
 177.mesa:       -Qipo -QxW  -O3 +FDO ONESTEP=yes
 178.galgel:     -Qipo -QxW  -O3 +FDO ONESTEP=yes
 179.art:        -Qipo -Oa -Qunroll4 -Zp4 ONESTEP=yes
 183.equake:     -Qipo -QxW  -Oa +FDO shlw32M.lib ONESTEP=yes
 187.facerec:    -Qipo -QxW  -O3 -Qunroll1 -Qscalar_rep- +FDO ONESTEP=yes
 188.ammp:       -QxW  -Oa ONESTEP=yes
 189.lucas:      -Qipo -QaxW
 191.fma3d:      basepeak=1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant BL20p G2 (3.06GHz/1MB L3 cache, Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1193 1160

SPEC license #: 3 Tested by:Hewlett-Packard Company, Houston TX Test date: Aug-2003 Hardware Avail: Jul-2003 Software Avail: Jun-2003

Notes/Tuning Information (Continued)

 200.sixtrack:   -Qipo -QxW  +FDO ONESTEP=yes
 301.apsi:       -Qipo -QxW  -O3 +FDO ONESTEP=yes