Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision Workstation 650 (3.2 GHz Xeon, 1MB L3 Cache)} SPECfp_rate2000 =

SPECfp_rate_base2000 =

18.3 18.2

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Sep-2003 Hardware Avail: Oct-2003 Software Avail: Apr-2003

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 5 10 15 20 25 30 35 168.wupwise 2 115 32.2 2 116 32.1

171.swim 2 482 14.9 2 482 14.9

172.mgrid 2 272 15.3 2 271 15.4

173.applu 2 361 13.5 2 360 13.5

177.mesa 2 109 29.9 2 109 29.8

178.galgel 2 225 29.8 2 226 29.7

179.art 2 628 9.61 2 602 10.0

183.equake 2 165 18.2 2 166 18.2

187.facerec 2 174 25.4 2 166 26.6

188.ammp 2 324 15.8 2 323 15.8

189.lucas 2 308 15.1 2 309 15.0

191.fma3d 2 252 19.4 2 252 19.4

200.sixtrack 2 188 13.6 2 183 13.9

301.apsi 2 343 17.6 2 341 17.7

Hardware

CPU: Intel Xeon (533 MHz system bus) CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: 1024KB(I+D) on chip Other Cache: N/A Memory: 4 x 512MB PC2100 ECC DDR SDRAM CL2-2-2 Disk Subsystem: 1 x 36GB 10K RPM U320 SCSI Other Hardware:

Software

Operating System: Windows XP Professional SP1 Compiler: Intel C++ Compiler 7.1 (20030402Z) Intel Fortran Compiler 7.1 (20030402Z) Microsoft Visual Studio .NET (7.0.9466) File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY
   178.galgel:   -FI /F32000000
 FEEDBACK DIRECTED OPTMIZATION
   ONESTEP=YES
   FDO:          PASS1=  -Qprof_gen  PASS2=-Qprof_use
 BASE TUNING
   C/F77/F90:    -Qipo -QxW -O3 +FDO
 PEAK TUNING
   168.wupwise:  -Qipo -QxW  -O3 +FDO
   171.swim:     -Qipo -QxW  -O3 +FDO
   172.mgrid:    -Qipo -QaxW -O3 +FDO
   173.applu:    -Qipo -QxW  -O3 -Qscalar_rep- -Qauto +FDO
   177.mesa:     -Qipo -QxW  -O3 -Oa +FDO
   178.galgel:   -Qipo -QxW  -O3 +FDO
   179.art:      -Oa -Qipo -Qunroll4 -Zp4
   183.equake:   -Qipo -QxW  -Oa -Qrcd +FDO
   187.facerec:  -O3 -QaxW -Qipo -Qunroll1 -Qscalar_rep- +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision Workstation 650 (3.2 GHz Xeon, 1MB L3 Cache)} SPECfp_rate2000 =

SPECfp_rate_base2000 =

18.3 18.2

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Sep-2003 Hardware Avail: Oct-2003 Software Avail: Apr-2003

Notes/Tuning Information (Continued)

   188.ammp:     -Oa -QxW
   189.lucas:    -Qipo -QaxW
   191.fma3d:    basepeak=yes
   200.sixtrack: -Qipo -QxW  +FDO
   301.apsi:     -Qipo -QxW  -O3 +FDO