Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL360 G4 (3.4GHz, Intel Xeon)

SPECint_rate2000 = SPECint_rate_base2000 =

16.3 15.9

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Jul-2004 Hardware Avail: Aug-2004 Software Avail: Aug-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 5 10 15 20 25 30 164.gzip 1 128 12.7 1 126 12.8

175.vpr 1 166 9.76 1 160 10.1

176.gcc 1 64.9 19.7 1 64.9 19.7

181.mcf 1 179 11.6 1 179 11.7

186.crafty 1 80.1 14.5 1 80.1 14.5

197.parser 1 147 14.2 1 147 14.2

252.eon 1 77.9 19.4 1 65.2 23.1

253.perlbmk 1 106 19.7 1 103 20.3

254.gap 1 65.1 19.6 1 64.1 19.9

255.vortex 1 80.5 27.4 1 80.5 27.4

256.bzip2 1 156 11.2 1 152 11.5

300.twolf 1 184 18.9 1 183 19.0

Hardware

CPU: Intel Xeon (3.4GHz, 1MB L2, 800MHz bus) CPU MHz: 3400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (HT Technology disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 16K micro-ops I + 16KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x1024MB PC2700 DDR-333 Disk Subsystem: 1x250GB SATA Other Hardware:

Software

Operating System: Windows Server 2003 Standard (Build 3790) Compiler: Intel C++ Compiler 8.0 Build 20031211Z

Microsoft Visual Studio .NET 7.0.9466 (for libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 +FDO*: FDO (-QxP not used in PASS1 to enable cross-compilation)
 Base tuning for C programs:   -QxP -fast +FDO* shlw32M.lib
 Base tuning for C++ programs: -QxP -fast -GX -GR
 Portability flags:
   176.gcc: -Dalloca=_alloca /F10000000
   186.crafy: -DNT_i386
   253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
   254.gap: -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 Peak tuning:
   164.gzip:    -QxP -fast -Oa           +FDO  ONESTEP=yes
   175.vpr:     -QxP -fast               +FDO  ONESTEP=yes
   176.gcc:     basepeak = 1
   181.mcf:     -QxP -fast               +FDO  ONESTEP=yes shlw32M.lib
   186.crafty:  -QxP -fast -Oa           +FDO  ONESTEP=yes shlw32M.lib
   197.parser:  -QxP -fast               +FDO  ONESTEP=yes
   252.eon:     -QxP       -O2 -Qipo     +FDO* ONESTEP=yes
   253.perlbmk:      -fast -Oa           +FDO  ONESTEP=yes shlw32M.lib
   254.gap:     -QxP -fast               +FDO  ONESTEP=yes
   255.vortex:  -QxP -fast               +FDO  ONESTEP=yes shlw32M.lib

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL360 G4 (3.4GHz, Intel Xeon)

SPECint_rate2000 = SPECint_rate_base2000 =

16.3 15.9

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Jul-2004 Hardware Avail: Aug-2004 Software Avail: Aug-2004

Notes/Tuning Information (Continued)

   256.bzip2:        -fast -Oa -Qunroll1 +FDO  ONESTEP=yes
   300.twolf:   -QxP -fast -O3           +FDO* shlw32M.lib
 BIOS Configuration Notes
   HT Technology disabled