Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers CELSIUS M430, Pentium 4 3.4F GHz

SPECfp2000 = SPECfp_base2000 =

1512 1507

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Aug-2004 Hardware Avail: Aug-2004 Software Avail: Mar-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 68.8 2326 68.8 2327

171.swim 3100 139 2226 139 2226

172.mgrid 1800 134 1348 133 1348

173.applu 2100 148 1415 143 1468

177.mesa 1400 93.6 1495 93.6 1495

178.galgel 2900 119 2435 119 2435

179.art 2600 200 1303 200 1303

183.equake 1300 75.2 1730 75.4 1725

187.facerec 1900 103 1836 103 1838

188.ammp 2200 213 1034 213 1034

189.lucas 2000 98.5 2030 98.7 2026

191.fma3d 2100 147 1431 147 1431

200.sixtrack 1100 181 609 179 616

301.apsi 2600 228 1141 228 1142

Hardware

CPU: Intel Pentium 4 (3.4F GHz, 800 MHz bus, Intel EM64T) CPU MHz: 3400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (HT Technology disabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 16KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2048 MB (4 512 MB PC2-4200, CL4, DDR2 ECC modules) Disk Subsystem: Maxtor 6Y160M0 (Serial ATA 7200 rpm) Other Hardware:

Software

Operating System: Windows XP Professional, Service Pack 1 Compiler: Intel(R) C++ Compiler, Version 8.0,

- Build 20040318Z Package ID: W_CC_PC_8.0.048 Intel(R) Fortran Compiler, Version 8.0 - Build 20040318Z Package ID: w_fc_pc_8.0.047 Microsoft Visual Studio .NET 7.0 (for libraries) MicroQuill SmartHeap Library 6.03a

File System: FAT32 System State: Default

Notes/Tuning Information

Portability flags:
178.galgel: -FI /F32000000

Feedback optimization:
  +FDO: PASS1= -Qprof_gen PASS2= -Qprof_use

 Baseline Tuning Flags:
 for C programs:
 -QxP -fast -Qansi_alias +FDO
 for Fortran programs:
 -QxP -fast -Qansi_alias +FDO

 Peak Tuning Flags:
 168.wupwise:  -QxP -fast -Qansi_alias +FDO
 171.swim:     basepeak=yes
 172.mgrid:    -QxP -fast -Qansi_alias +FDO
 173.applu:  -QxP -fast -Qscalar_rep- -Qauto  +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers CELSIUS M430, Pentium 4 3.4F GHz

SPECfp2000 = SPECfp_base2000 =

1512 1507

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Aug-2004 Hardware Avail: Aug-2004 Software Avail: Mar-2004

Notes/Tuning Information (Continued)

 177.mesa:   -QxP -fast -Oa -Qscalar_rep- +FDO
 178.galgel:     basepeak=yes
 179.art:      basepeak=yes
 183.equake:   -QxP -Oa -Qrcd -Qipo +FDO
 187.facerec:  -QxP -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     basepeak=yes
 189.lucas:    -QxP -fast -Qprefetch- +FDO
 191.fma3d:    basepeak=yes
 200.sixtrack: -Qipo -QxP +FDO
 301.apsi:     -QxP -fast +FDO

For information about Fujitsu Siemens Computers in your country please see:
http://www.fujitsu-siemens.com/countries