Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY BX630, AMD Opteron (TM) 850

SPECfp_rate2000 = SPECfp_rate_base2000 =

35.4 35.4

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Sep-2005 Hardware Avail: Oct-2005 Software Avail: Jun-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 80 90 168.wupwise 2 66.7 55.6 2 66.7 55.6

171.swim 2 172 41.9 2 172 41.9

172.mgrid 2 126 33.2 2 126 33.2

173.applu 2 166 29.4 2 166 29.4

177.mesa 2 152 21.3 2 152 21.3

178.galgel 2 115 58.4 2 115 58.4

179.art 2 69.6 86.7 2 69.6 86.7

183.equake 2 89.7 33.6 2 89.7 33.6

187.facerec 2 112 39.2 2 112 39.2

188.ammp 2 205 24.9 2 205 24.9

189.lucas 2 132 35.2 2 132 35.2

191.fma3d 2 153 31.9 2 153 31.9

200.sixtrack 2 151 16.9 2 151 16.9

301.apsi 2 193 31.2 2 193 31.2

Hardware

CPU: AMD Opteron (TM) 850 processor (2.40 GHz) CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 8x2048MB DDR-RAM PC3200R Disk Subsystem: Seagate ST3160023AS (SATA, 7.2krpm) Other Hardware: None

Software

Operating System: Windows Server 2003 Enterprise Edition + SP1 Compiler: PGI Fortran compiler 6.0-4 for Windows XP,

PGI C compiler 6.0-4 for Windows XP

File System: NTFS System State: Default

Notes/Tuning Information

 GENERAL
 +FDO: PASS1=-Mpfi  PASS2=-Mpfo
 ONESTEP is set to 1 for every compile with the PGI compilers.

 Portability flags
    178.galgel: -Mfixed

 Base tuning flags
    for Fortran programs: -fastsse -Mipa=fast,inline +FDO
    for C programs:       -fastsse -Mipa=fast,inline

 Peak tuning flags
    same as baseline (basepeak=yes set globally)

 ’start /b /wait /affinity’ command is used to bind CPU(s) to processes
 boot options: /NoExecute=alwaysoff

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY BX630, AMD Opteron (TM) 850

SPECfp_rate2000 = SPECfp_rate_base2000 =

35.4 35.4

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Sep-2005 Hardware Avail: Oct-2005 Software Avail: Jun-2005

Notes/Tuning Information (Continued)

 This result was measured with 32-bit binaries using the 32-bit version of
 the operating system.

 For information about Fujitsu Siemens Computers in your country please see:
 http://www.fujitsu-siemens.com/countries