Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer xSeries 306m (3.2 GHz Pentium 4 640, 2MB L2 Cache)

SPECint2000 = SPECint_base2000 =

1593 1585

SPEC license #: 11 Tested by: IBM Corporation Test date: Aug-2005 Hardware Avail: Sep-2005 Software Avail: Jun-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 132 1060 131 1069

175.vpr 1400 128 1096 124 1125

176.gcc 1100 58.4 1883 58.4 1883

181.mcf 1800 90.0 2001 89.9 2001

186.crafty 1000 84.3 1187 84.6 1182

197.parser 1800 134 1343 133 1348

252.eon 1300 64.6 2011 64.9 2004

253.perlbmk 1800 94.0 1916 93.4 1928

254.gap 1100 63.9 1723 62.3 1766

255.vortex 1900 70.3 2703 70.3 2701

256.bzip2 1500 123 1222 123 1223

300.twolf 3000 183 1638 183 1638

Hardware

CPU: Intel Pentium 4 640(800 MHz system bus) CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12K(I) micro-ops + 16KB(D) on chip Secondary Cache: 2048KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4 x 1024 MB ECC PC2-3200 Single Rank Disk Subsystem: 75GB SATA 7.2K RPM Other Hardware:

Software

Operating System: Windows Server 2003 Standard Edition Compiler: Intel C/C++ Compiler 9.0 (20050624Z) for 32-bit applications

Intel Fortran Compiler 9.0 (20050624Z) for 32-bit applications Microsoft Visual Studio .NET 13.0.9466 (for libraries) MicroQuill Smartheap Library 7.30

File System: NTFS System State: Default

Notes/Tuning Information

 GENERAL
   ONESTEP=yes
   +FDO:   PASS1=-Qprof_gen  PASS2=-Qprof_use
 PORTABILITY FLAGS
   176.gcc:     -Dalloca=_alloca /F10000000
   186.crafty:  -DNT_i386
   252.eon:    srcalt=stdcpp
   253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
   254.gap:     -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 BASE TUNING
   C:           -fast -Qansi_alias +FDO shlW32M.lib
   C++:         -fast -Qcxx_features +FDO
 PEAK TUNING
   164.gzip:    -fast +FDO
   175.vpr:     -fast +FDO
   176.gcc:     basepeak=yes
   181.mcf:     -fast +FDO shlW32M.lib
   186.crafty:  -fast -Oa +FDO shlW32M.lib
   197.parser:  -fast +FDO
   252.eon:     -fast +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer xSeries 306m (3.2 GHz Pentium 4 640, 2MB L2 Cache)

SPECint2000 = SPECint_base2000 =

1593 1585

SPEC license #: 11 Tested by: IBM Corporation Test date: Aug-2005 Hardware Avail: Sep-2005 Software Avail: Jun-2005

Notes/Tuning Information (Continued)

   253.perlbmk: -fast -Oa +FDO shlW32M.lib
   254.gap:     -fast +FDO
   255.vortex   -fast +FDO shlw32M.lib
   256.bzip2:   -fast -Qunroll1 -Oa +FDO shlw32M.lib
   300.twolf:   -fast +FDO shlW32M.lib
 EXTRA LIBRARIES
   shlW32M.lib: MicroQuill SmartHeap Library 7.3
                www.microquill.com