Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Acer Incorporated

Altos G5350 (AMD Opteron (TM) 246)

SPECfp2000 = SPECfp_base2000 =

1526 1413

SPEC license #: 97 Tested by: Acer Incorporated Test date: Oct-2005 Hardware Avail: Jul-2005 Software Avail: Jun-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 73.5 2176 74.2 2156

171.swim 3100 157 1978 156 1989

172.mgrid 1800 140 1287 140 1287

173.applu 2100 169 1245 160 1313

177.mesa 1400 185 758 94.5 1482

178.galgel 2900 124 2346 114 2553

179.art 2600 72.5 3589 72.5 3589

183.equake 1300 92.5 1405 91.3 1424

187.facerec 1900 120 1585 120 1586

188.ammp 2200 229 960 199 1106

189.lucas 2000 128 1563 114 1747

191.fma3d 2100 166 1264 164 1278

200.sixtrack 1100 181 609 180 610

301.apsi 2600 233 1115 234 1113

Hardware

CPU: AMD Opteron (TM) 246 CPU MHz: 2000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4 x 1024MB, DDR400 CL3 ECC Disk Subsystem: 1 x 36GB 10000RPM U320 SCSI HDD Other Hardware: None

Software

Operating System: Microsoft Windows Server 2003 Enterprise Edition (Build 3790) Compiler: Intel C++ 9.0 build 20050430Z for IA32

Intel Fortran 9.0 build 20050722Z for IA32 PGI Fortran compiler 6.0-5 PGI C compiler 6.0-5 ACML Version 2.5.3 (bundled with PGI 6.0-5)

File System: NTFS System State: default

Notes/Tuning Information

  +FDO:
   icl, ifort  : PASS1=-Qprof_gen  PASS2=-Qprof_use
   pgf90       : PASS1=-Mpfi       PASS2=-Mpfo
  ifort is the Intel Fortran compiler, icl is the Intel C++ compiler and
  pgf90 is the PGI Fortran 90 compiler.
  pgcc is the PGI C compiler.
  ONESTEP is set to 1 for every compile with the PGI compilers.
  Portability:
  178.galgel:                 -Mfixed
  Baseline: C      :  pgcc    -fastsse -Mipa=fast,inline
  Baseline: Fortran:  pgf90   -fastsse -Mipa=fast,inline +FDO
  Peak tuning:
  168.wupwise:        pgf90   -fastsse -Mipa=fast,inline -Mnovect
  171.swim:           ifort   -Qipo  -O3  -QaxN -QxW -Qunroll0 +FDO
  172.mgrid:          pgf90   -fastsse -Mipa=fast,inline
  173.applu:          ifort   -Qipo  -O3 -QaxN -QxW -auto +FDO
  177.mesa:           icl     -Qipo -arch:SSE2 -Qunroll1 -Qansi_alias +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Acer Incorporated

Altos G5350 (AMD Opteron (TM) 246)

SPECfp2000 = SPECfp_base2000 =

1526 1413

SPEC license #: 97 Tested by: Acer Incorporated Test date: Oct-2005 Hardware Avail: Jul-2005 Software Avail: Jun-2005

Notes/Tuning Information (Continued)

                              -Qoption,f,-ip_ninl_max_stats=1500,-ip_ninl_max_total_stats=4500
  178.galgel:         pgf90   -fastsse -Mipa=fast,safe RM_SOURCES=lapak.f90
                              -Munix -lacml
  179.art:            pgcc     basepeak=yes
  183.equake:         icl     -fast -arch:SSE2 -QaxW +FDO
  187.facerec:        pgf90   -fastsse -Mipa=fast,inline +FDO
  188.ammp:           icl     -Oa   -arch:SSE2  -Zp4 -Qansi_alias
  189.lucas:          ifort   -Qipo -QxW -Qunroll1
  191.fma3d:          pgf90   -Mipa=fast,inline -fastsse -Mnovect +FDO
  200.sixtrack:       pgf90   -fastsse -Mipa=fast,inline
  301.apsi:           pgf90   -fastsse -Mipa=fast,inline