Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL580 G4 (3.0GHz, Intel Xeon processor 7041)

SPECfp_rate2000 = SPECfp_rate_base2000 =

28.5 28.4

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: May-2006 Hardware Avail: May-2006 Software Avail: May-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 168.wupwise 2 75.5 49.2 2 75.6 49.1

171.swim 2 283 25.4 2 283 25.4

172.mgrid 2 182 22.9 2 182 22.9

173.applu 2 217 22.4 2 217 22.4

177.mesa 2 110 29.5 2 110 29.7

178.galgel 2 108 62.0 2 108 62.0

179.art 2 103 58.6 2 103 58.6

183.equake 2 90.9 33.2 2 90.8 33.2

187.facerec 2 159 27.7 2 159 27.7

188.ammp 2 251 20.3 2 239 21.4

189.lucas 2 196 23.7 2 196 23.7

191.fma3d 2 218 22.3 2 218 22.3

200.sixtrack 2 188 13.6 2 187 13.6

301.apsi 2 255 23.7 2 255 23.7

Hardware

CPU: Intel Xeon processor 7041 (3.0GHz, 2x2MB L2, 800MHz bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 12K micro-ops I + 16KBD (on chip) per core Secondary Cache: 2048KB(I+D) (on chip) per core L3 Cache: N/A Other Cache: N/A Memory: 8x2048MB PC2-3200 dual-rank Disk Subsystem: 1x36GB SAS Other Hardware:

Software

Operating System: Windows Server 2003 Enterprise SP1 Compiler: Intel C++ Compiler for 32-bit applications,

(Version 9.1 Build 20060323Z) Intel Fortran Compiler for 32-bit applications, (Version 9.1 Build 20060323Z) Microsoft Visual Studio .NET 7.0.9466 (for libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use

 Base tuning for Fortran programs: -fast -Qansi_alias +FDO
 Base tuning for C programs:       -fast              +FDO shlw32M.lib
 Portability flags:
   178.galgel: -FI /F32000000
 Peak tuning:
   168.wupwise:  -fast -Qansi_alias                 +FDO
   171.swim:     -fast                              +FDO ONESTEP=yes
   172.mgrid:    -fast -Qansi_alias                 +FDO
   173.applu:    basepeak=1
   177.mesa:     -fast                              +FDO ONESTEP=yes
   178.galgel:   basepeak=1
   179.art:      basepeak=1
   183.equake:   -fast -Oa -Qrcd                    +FDO ONESTEP=yes shlw32M.lib
   187.facerec:  -fast -Qunroll1 -Qscalar_rep-      +FDO ONESTEP=yes
   188.ammp:     -fast -Qansi_alias                 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL580 G4 (3.0GHz, Intel Xeon processor 7041)

SPECfp_rate2000 = SPECfp_rate_base2000 =

28.5 28.4

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: May-2006 Hardware Avail: May-2006 Software Avail: May-2006

Notes/Tuning Information (Continued)

   189.lucas:    -fast
   191.fma3d:    basepeak=1
   200.sixtrack: -fast                              +FDO
   301.apsi:     basepeak=1
 BIOS Configuration Notes
   Hyper-Threading Technology disabled