Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEQUEST 580

SPECint_rate2000 = SPECint_rate_base2000 =

1016 1016

SPEC license #: 19 Tested by: Fujitsu Limited Test date: Jul-2006 Hardware Avail: Aug-2006 Software Avail: May-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 500 1000

1500

2000

164.gzip 64 141 739 64 141 739

175.vpr 64 124 839 64 124 839

176.gcc 64 65.9 1239 64 65.9 1239

181.mcf 64 73.7 1814 64 73.7 1814

186.crafty 64 79.6 933 64 79.6 933

197.parser 64 177 754 64 177 754

252.eon 64 58.8 1643 64 58.8 1643

253.perlbmk 64 132 1012 64 132 1012

254.gap 64 168 487 64 168 487

255.vortex 64 90.9 1551 64 90.9 1551

256.bzip2 64 121 918 64 121 918

300.twolf 64 207 1075 64 207 1075

Hardware

CPU: Dual Core Intel(R) Itanium(R) 2 (1.6GHz/24MB, 533MHz FSB) CPU MHz: 1600 FPU: Integrated CPU(s) enabled: 64 cores, 32 chips, 2 cores/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1-32(chips) Parallel: no Primary Cache: 16KBI + 16KBD on chip, per core Secondary Cache: 1024KBI + 256KBD on chip, per core L3 Cache: 12.0MB (I+D) on chip, per core Other Cache: N/A Memory: 256GB (256x1GB DIMMs) Disk Subsystem: Fujitsu MAT3073NC (SCSI Ultra 320) Other Hardware: N/A

Software

Operating System: Red Hat Enterprise Linux AS 4 Update2 Compiler: Intel(R) C++ Compiler for Linux 9.1 (Build 20060523) File System: ext2 System State: Single-user

Notes/Tuning Information

 +FDO: PASS1=-prof-gen PASS2=-prof-use
 Baseline optimization flags:
   C programs:       -fast -auto-ilp32 -IPF-fp-relaxed +FDO
   C++ programs:     -fast -ansi-alias -IPF-fp-relaxed +FDO
 Peak optimization flags:
   same as base (basepeak=true)

 Processes are bound to CPUs using taskset.
 Memory system is in "Non Mirror Mode".

 Portability Flags:
   176.gcc     : -DSPEC_CPU2000_LP64 -Dalloca=_alloca
   186.crafty  : -DLINUX_i386
   252.eon     : -DSPEC_CPU2000_LP64 -DHAS_ERRLIST
   253.perlbmk : -DSPEC_CPU2000_LP64 -DSPEC_CPU2000_NEED_BOOL
                 -DSPEC_CPU2000_LINUX_IA64
   254.gap     : -DSPEC_CPU2000_LP64 -DSYS_HAS_CALLOC_PROTO -DSYS_IS_USG
                 -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                 -DSYS_HAS_SIGNAL_PROTO -include unistd.h
   255.vortex  : -DSPEC_CPU2000_LP64