Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL140 G3 (3.0 GHz, Intel Xeon processor 5160)

SPECfp2000 = SPECfp_base2000 =

2933 2719

SPEC license #: 2323 Tested by: QLogic Corporation Test date: Nov-2006 Hardware Avail: Jun-2006 Software Avail: Aug-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 5000 10000 15000

168.wupwise 1600 49.2 3250 47.2 3388

171.swim 3100 124 2509 124 2509

172.mgrid 1800 91.8 1961 88.6 2031

173.applu 2100 88.5 2373 74.9 2803

177.mesa 1400 44.0 3184 40.9 3424

178.galgel 2900 42.1 6892 35.5 8175

179.art 2600 23.1 11249 21.0 12399

183.equake 1300 65.6 1983 59.4 2189

187.facerec 1900 40.5 4693 38.8 4897

188.ammp 2200 118 1859 106 2083

189.lucas 2000 81.5 2454 77.3 2589

191.fma3d 2100 118 1774 118 1774

200.sixtrack 1100 107 1026 95.5 1152

301.apsi 2600 156 1667 148 1760

Hardware

CPU: Intel Xeon processor 5160 (1333 MHz system bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 1,2 chips Parallel: No Primary Cache: 32KBI + 32KBD on chip, per core Secondary Cache: 4MB (I+D) on chip, per chip L3 Cache: N/A Other Cache: N/A Memory: 4 GB (4 x 1 GB PC2-5300F) Disk Subsystem: SATA, 60 GB Other Hardware: None

Software

Operating System: SUSE Linux Enterprise Server 10 (x86_64) Compiler: QLogic PathScale Fortran and C Compilers, Release 2.5 Intel Math Kernel Library 8.1 compat-libstdc++5 for SLES 10 File System: ext2 System State: Multi-user, run level 3

Notes/Tuning Information

Tested by QLogic Corporation
 +FDO: PASS1= -fb_create fbdata  PASS2= -fb_opt fbdata
 +MKL means linking with Intel Math Kernel Library 8.1 with these LD flags:
      -L$(SPEC)/mkl -lmkl_lapack -lmkl
 Base tuning for C programs:       -Ofast -WOPT:mem_opnds=on -march=core +FDO
 Base tuning for FORTRAN programs: -Ofast -LNO:fusion=2 -march=core +FDO
 Portability flags:
   178.galgel:    -fixedform
 Peak tuning:
   168.wupwise:   -Ofast -LNO:fusion=2 -OPT:unroll_size=0
                  -CG:local_fwd_sched=on -march=core
   171.swim:      basepeak=yes
   172.mgrid:     -Ofast -LNO:blocking=off:fusion=2 -march=core
   173.applu:     -Ofast -LNO:fission=1:fusion=2:full_unroll_size=9000
                  -OPT:treeheight=on:unroll_size=0 -march=core
   177.mesa:      -O2 -ipa -IPA:plimit=20000 -WOPT:aggstr=0
                  -march=core +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL140 G3 (3.0 GHz, Intel Xeon processor 5160)

SPECfp2000 = SPECfp_base2000 =

2933 2719

SPEC license #: 2323 Tested by: QLogic Corporation Test date: Nov-2006 Hardware Avail: Jun-2006 Software Avail: Aug-2006

Notes/Tuning Information (Continued)

   178.galgel:    -Ofast -CG:load_exe=1:local_fwd_sched=on:prefetch=off
                  -OPT:early_intrinsics=on -march=core +MKL
                   RM_SOURCES= lapak.f90
   179.art:       -Ofast -WOPT:mem_opnds=on:unroll=2 -march=core
   183.equake:    -Ofast -OPT:treeheight=on -m32 -march=core +FDO
   187.facerec:   -Ofast -IPA:plimit=1500 -LNO:fusion=2
           -OPT:IEEE_NaN_Inf=off:ro=3:unroll_size=0 -march=core +FDO
   188.ammp:      -O3 -OPT:IEEE_arith=3:Ofast:alias=disjoint -ffast-math
                  -march=core
   189.lucas:     -Ofast -CG:load_exe=2 -LNO:fusion=0 -march=core
   191.fma3d:     basepeak=yes
   200.sixtrack:  -O3 -CG:cflow=off -OPT:Ofast:early_intrinsics=on
                  -march=core +FDO
   301.apsi:      -Ofast -LNO:opt=0 -march=core

 Taskset utility used to bind process to CPU(s)