Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp^®_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

Copies

SPECfp_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

0 115

5.00 10.0 15.0 20.0 25.0 30.0 35.0 40.0 45.0 50.0 55.0 60.0 65.0 70.0 75.0 80.0 85.0 90.0 95.0 100 105 110 63 89.5

63 57.4

63 59.4

63 81.8

63 70.2

63 57.5

63 58.6

63 57.9

63 59.6

63 57.0

48 59.7

63 65.5

63 66.5

63 102 63 106

63 70.0

63 88.1

63 114

63 43.5

63 51.4

63 56.5

56 62.5

63 30.2

8 51.4

63 72.6

63 73.7

63 82.2

63 84.6

Hardware

CPU Name: UltraSPARC T2 CPU Characteristics: CPU MHz: 1582 FPU: Integrated CPU(s) enabled: 8 cores, 1 chip, 8 cores/chip, 8 threads/core CPU(s) orderable: 1 chips Primary Cache: 16 KB I + 8 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip

Software

Operating System: Solaris 10 10/08 Compiler: Sun Studio 12 and gccfss V4.2.1 (see additional detail below) Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit

Continued on next page Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5 SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008 L3 Cache: None Other Cache: None Memory: 64 GB (16 x 4 GB) Disk Subsystem: 142 GB Solaris Volume Manager RAID 0 on 4x 72 GB Sun 10K RPM SAS block size 384 KB Other Hardware: None

Other Software: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 63 9523 89.9 9574 89.4 9571 89.5 63 9523 89.9 9574 89.4 9571 89.5 416.gamess 63 21500 57.4 21484 57.4 21495 57.4 63 20761 59.4 20765 59.4 20767 59.4 433.milc 63 7066 81.8 7067 81.8 7064 81.9 63 7066 81.8 7067 81.8 7064 81.9 434.zeusmp 63 8186 70.0 8133 70.5 8164 70.2 63 8186 70.0 8133 70.5 8164 70.2 435.gromacs 63 7806 57.6 7818 57.5 7871 57.1 63 7679 58.6 7677 58.6 7713 58.3 436.cactusADM 63 12977 58.0 13023 57.8 13005 57.9 63 12664 59.4 12622 59.6 12614 59.7 437.leslie3d 63 10422 56.8 10384 57.0 10372 57.1 48 7569 59.6 7553 59.7 7543 59.8 444.namd 63 7729 65.4 7713 65.5 7714 65.5 63 7598 66.5 7633 66.2 7598 66.5 447.dealII 63 7096 102 7110 101 7091 102 63 6805 106 6787 106 6772 106 450.soplex 63 7515 69.9 7500 70.1 7506 70.0 63 7515 69.9 7500 70.1 7506 70.0 453.povray 63 3877 86.4 3803 88.1 3806 88.1 63 2989 112 2942 114 2923 115 454.calculix 63 11931 43.6 11950 43.5 11936 43.5 63 11931 43.6 11950 43.5 11936 43.5 459.GemsFDTD 63 12996 51.4 12993 51.4 12994 51.4 63 12996 51.4 12993 51.4 12994 51.4 465.tonto 63 10891 56.9 10981 56.5 10990 56.4 56 8791 62.7 8812 62.5 8867 62.1 470.lbm 63 28620 30.2 28613 30.3 28627 30.2 8 2139 51.4 2139 51.4 2140 51.4 481.wrf 63 9690 72.6 9700 72.5 9682 72.7 63 9540 73.8 9566 73.6 9544 73.7 482.sphinx3 63 14916 82.3 14940 82.2 14961 82.1 63 14518 84.6 14512 84.6 14518 84.6

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Invocation Notes

 Sun Studio compiler patches are available at
 http://developers.sun.com/sunstudio/downloads/patches/ss12_patches.jsp
 The tested configuration included patch 124867-08, 124861-09,
 124863-08, 127000-06

 Peak also uses "GCC for SPARC Systems 4.2.1", which
 combines gcc with the Sun Code Generator for SPARC
 systems.  It is invoked as "gcc", and accepts source
 code compatible with GCC 4.2.
 For more information, including support, see
      http://cooltools.sunsource.net/gcc/

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

Submit Notes

 A processor set was created using
   psrset -c 1-63
 and the runspec process was placed into the set using
   psrset -e 1
 The config file option ’submit’ was used to select specific
 processors within the set, along with the pbind command.

Operating System Notes

 ulimit -s 131072 was used to allow the stack to grow
 up to 131072 KB (aka 128 MB).  Note that saying "131072"
 is preferable to "unlimited", because there is a tradeoff
 between space for the stack vs. space for the heap.

 /etc/system parameters
    autoup=600
       Causes pages older than the listed number of seconds to
       be written by fsflush.
    bufhwm=3000
       Memory byte limit for caching I/O buffers
    segmap_percent=1
       Set maximum percent memory for file system cache
    tune_t_fsflushr=10
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush.
    tsb_rss_factor=128
       Suggests that the the size of the TSB (Translation Storage Buffer)
       may be increased if it is more than 25% (128/512) full.  Doing so
       may reduce TSB traps, at the cost of additional kernel memory.

 The "webconsole" service was turned off using
     svcadm disable webconsole

 The system had 75 GB of swap space.

Platform Notes

 This result was measured on a Sun SPARC Enterprise
 T5220.  All of these are electronically equivalent:
   - Sun SPARC Enterprise T5120
   - Sun SPARC Enterprise T5220
   - Fujitsu SPARC Enterprise T5120
   - Fujitsu SPARC Enterprise T5220
 A SPARC Enterprise 5120 can hold up to 4 disks, and a
 5220 can hold up to 8.  This system was tested with 4
 disks; therefore, this result applies to both the 5120
 and the 5220.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Base Optimization Flags

C benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2 -xalias_level=std
-xprefetch_level=3 -xprefetch_auto_type=indirect_array_access
-M /usr/lib/ld/map.bssalign

C++ benchmarks:

-g0 -library=stlport4 -fast -xipo=2 -xpagesize=4M -xprefetch_level=2
-xdepend -xalias_level=compatible -M /usr/lib/ld/map.bssalign

Fortran benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2
-M /usr/lib/ld/map.bssalign

Benchmarks using both Fortran and C:

-g -fast(cc) -fast(f90) -xipo=2 -xpagesize=4M -xprefetch_level=2
-xalias_level=std -xprefetch_level=3
-xprefetch_auto_type=indirect_array_access -M /usr/lib/ld/map.bssalign

Base Other Flags

C benchmarks:

-xjobs=32 -V -#

C++ benchmarks:

-xjobs=32 -verbose=diags,version

Fortran benchmarks:

-xjobs=32 -V -v

Benchmarks using both Fortran and C:

-xjobs=32 -V -# -v

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks (except as noted below):

CC

447.dealII: g++

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Peak Optimization Flags

C benchmarks:

433.milc: basepeak = yes

470.lbm: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xprefetch_level=3 -xipo=2
-xrestrict

482.sphinx3: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xinline= -xprefetch_level=2
-Wc,-Qlp-ol=1 -xrestrict -xalias_level=strong -fsimple=1
-xlinkopt=2 -lfast

C++ benchmarks:

444.namd: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xdepend -xalias_level=compatible
-M /usr/lib/ld/map.bssalign -xprefetch_level=1 -xlinkopt=2

447.dealII: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xdepend -Wl,-M,/usr/lib/ld/map.bssalign -xipo=2 -xrestrict
-xalias_level=std

450.soplex: basepeak = yes

453.povray: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=64K
-xdepend -xalias_level=compatible -xipo=2 -xrestrict
-xlinkopt=2

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5

SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

Peak Optimization Flags (Continued)

Fortran benchmarks:

410.bwaves: basepeak = yes

416.gamess: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xlinkopt=2

434.zeusmp: basepeak = yes

437.leslie3d: -g -fast -xpagesize_heap=4M -xpagesize_stack=64K

-M /usr/lib/ld/map.bssalign -xprefetch_level=3
-xprefetch=latx:1.6 -qoption cg -Qlp=1 -qoption cg -Qlp-fa=0
-qoption cg -Qlp-fl=1 -qoption cg -Qlp-av=448
-qoption cg -Qlp-t=4

459.GemsFDTD: basepeak = yes

465.tonto: -g -fast -xpagesize=4M -M /usr/lib/ld/map.bssalign -xipo=2

-lfast

Benchmarks using both Fortran and C:

435.gromacs: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xipo=1 -xinline=
-xarch=generic -xchip=generic -fsimple=0

436.cactusADM: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xipo=2
-fsimple=1 -xlinkopt=2

454.calculix: basepeak = yes

481.wrf: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xlinkopt=2

Peak Other Flags

C benchmarks:

-xjobs=32 -V -#

C++ benchmarks (except as noted below):

-xjobs=32 -verbose=diags,version

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 7 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise T5120

SPECfp_rate2006 = 68.5 SPECfp_rate_base2006 = 64.1

CPU2006 license: 6 Test date: Jan-2009 Test sponsor: Sun Microsystems Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Nov-2008

Peak Other Flags (Continued)

447.dealII: -v

Fortran benchmarks:

-xjobs=32 -V -v

Benchmarks using both Fortran and C:

-xjobs=32 -V -# -v

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-12u1-and-gccfss4.2.r3.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-12u1-and-gccfss4.2.r3.xml

Originally published on 5 August 2009.

Report generated on Wed Jul 23 03:11:42 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance